### DCC XYZ_0

Provides the default "X" or "R" (radius) value for the center location for all auto features except a line where it defines the start point. The value will represent X value when the "Cartesian" value is set to TRUE (1), and R when it is set to FALSE (0). This value and the "DccXYZ_1" and "DccXYZ_2" values are used for Contact probes while the "Point1(XYZ)" values are used for Vision and Laser probes.

Entry Name: DccXYZ_0

Entry Type: Real Number to specify the X or R value. Default value is 0.