### DMIS Use Chorus Wrist Rotation

This option should be turned on if you are using a DEA CMM equipped with an IW42, CW43 or CW43L wrist. PC-DMIS follows Chorus conventions and adjusts the B rotation angle during the import of the SNSLCT statement. This option is automatically used when performing a ChorusDMIS import.

Entry Name: DMISUseChorusWristRotation

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.