### Maximum Arc Segment Radius In MM

This value is used to control the maximum radius for an arc segment that is created from the segmentation process of a continuous scan. PC-DMIS uses internal functions to create line and arc segments that make up a continuous scan. Arc segments that have a larger radius than this value will be eliminated from the scan data. This settings as well as the "MinimumArcSegmentRadiusInMM" and "MinimumLineSegmentLengthInMM" settings help deal with noise in the scan line and provide more consistent segmentation.

Entry Name: MaximumArcSegmentRadiusInMM

Entry Type: Real Number specifying maximum segment radius. Default value is 2000.