### Sensor CG Loc Type

This is used for persistent storage of the default value of the CG Locator, as described in the Laser Documentation. See the "Laser Probe Toolbox: Laser Pixel Locator Properties tab" topic in the PC-DMIS Laser documentation for more information.

Entry Name: SensorCGLocType

Entry Type: Whole Number specifying Locator type. Default value is 0.

CG Locator Type Key:

0 | Brightest
1 | Fixed Threshold
2 | Gradient