### DCC Thickness 2 Is Actual

This option determines how the thickness distance that is provided by the "DccThickness2Distance" is applied. This is applied for Auto Edge Points.

- 0 - Adjust Theoretical option should be used when the theoretical values need to be adjusted by a thickness because measurements are being done on opposite side of material.

- 1 - Adjust Actual option should be used when measurements are being adjusted by the thickness back to the original theoretical XYZ locations. With this option it will appear that the theoretical and measured values have not been offset and the target is offset. You still need to modify your target so that PC-DMIS drives to the correct location.

Entry Name: DCCThickness2IsActual

Entry Type: Whole Number to specify thickness option. Default value is 0.