#### Focus Graph

Auto focus will graph the results of the focus by showing the focus score (Y) against time (X). A sharper focus will have a higher focus score.

Auto focus should result in a rounded curve (an inverted "U"). Use the Manual Focus option when you have no DCC to automatically drive the Z axis. If the graph shows a sharp increase in focus score, try reducing the speed of movement. Also, you need to ensure that your range of travel is sufficient so you see the base of the curve on both sides.

If the graph is not smooth, ensure the illumination is sufficient so that surface texture is evident.

Auto Focus on a Manual Machine:

1. Roughly find the in-focus position, and then move out of focus.

2. Click the Auto Focus button to start the graph and record the focus score.

3. Move through the focus position by moving a single axis (usually Z).

4. Continue moving the Z axis until you have moved through the focus position, and the graph is a well-proportioned, gradual, inverted U shape.

5. When the specified duration has been reached, the detected focus position will be displayed in the live image view.

6. A message is displayed to accept the focus, or retry.

7. Click the Reset Focus Graph button to clear the graph data and start this process over if there is a problem.

Note: With focus on a manual machine, you need to move the Z stage at a slow and steady speed. You will be warned if you move too fast, or the distance moved was too long or too short.
On some machines, you may find you get a better focus result by specifying a longer duration and moving forward and backward through the focus position 3 or 4 times to get a series of U shapes on the graph.