### Calibrating NC-100 Video Probes

You will need to calibrate this probe on a special polyhedral calibration tool that has 17 faces, requiring 17 orientations of the probe head. You will also need to utilize a calibrated touch trigger probe to calibrate the orientation of the polyhedral tool.

Important! The entire NC-100 Video Probe calibration process takes about one hour to perform. Be sure to allow enough time to complete the process. Segmenting this procedure may result in having to start the process from the beginning.

You will need two types of calibration tools: A sphere calibration tool and a polyhedral calibration tool.

More:

Calibrate the Touch Trigger Probe:

Calibrate NC100 Video Probe