## Getting Started

There are a few basic steps that you should take to verify that your system has been properly prepared before using PC-DMIS Vision with your Vision machine.

Note: You will get the best measurement results if your optical measuring system is setup in a dimly lit room that doesn't have a lot of uncovered windows or bright lights with little temperature variation.

Follows these steps to get started with PC-DMIS Vision:

- Step 1: Install and Launch PC-DMIS Vision

- Step 2: Home your System

- Step 3: Create a Vision Probe File

- Step 4: Edit your Vision Tip

- Step 5: Perform Calibrations

- Step 6: Modify Machine Options

- Frame Grabber