## Appendix C: Using the NC-100 Video Probe

This appendix deals specifically with using a NC-100 Video Probe with PC-DMIS Vision. The NC-100 video probe is considered a "non-contact probe". This means the probe never touches the part while taking measurements. The following topics in the PC-DMIS Core documentation that deal with general NC-100 options:

- Setup Options: NC-100 Setup tab

- Parameter Settings: NC-100 Parameters tab

The following topics are discussed in this appendix:

- Calibrating NC 100 Video Probes

- Measuring Auto Features with the NC-100 Video Probe