### Cylinder Centering Thread Scan Strategy

This measurement strategy for the Cylinder Auto Feature type performs a thread scan by maintaining the probe centered within the thread.

To perform a single scan, see Working with Measurement Strategies.

Note: When using this strategy, the diameter of the probe tip must exceed the size of the valleys in-between the threads in order to prevent probe shanking.