#### Cylinder Basic Scan - Key In Method

This method lets you type the X, Y and Z value of the cylinder's centroid, and vectors.

1. Double-click the centroid point in the List Box in the ‘#’ column. This will display the Edit Scan Item dialog box. The title bar of the dialog box displays the ID of the specific parameter being edited.

Edit Scan Item dialog box

2. Manually edit the X, Y, or Z value.

3. Click the OK button to apply the changes.

The Cancel button will disregard any changes that have been made and will close the dialog box.

You should also key-in the CutVec and the InitVec of the cylinder using this same process.