### Auto Adjust TesaM 5 Degrees

When this option is set to TRUE (1), PC-DMIS automatically switches the set active tip commands to the closest A and B angles based on the index increment. This works for part programs written for either a Tesastar M or PH10 probe and then run on a machine with the other probe type.

This facilitates the use of angles that are not available on the other machine. The probe files will be different on the two machines but should have the same names. A message should appear with a list of angles that have been converted (if any).

Entry Name: AutoAdjustTesaM5Degrees

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1.