### Probe Qual Analog Disk Bottom Hits Distance From Edge

During disk calibration on an analog probe, PC-DMIS measures the bottom of the disk. Defines the distance in millimeters from the outer edge of the bottom of the disk at which PC-DMIS takes hits.

Entry Name: ProbeQualAnalogDiskBottomHitsDistancefromEdge

Entry Type: Real number specifying distance. The default is 2.

Note: In PC-DMIS 2012 MR1 and higher, the ProbeQualAnalogDiskBottomHitsDistanceFromEdge registry setting provides the initial defaults for new probes. You can then define specific settings for individual probes in the Edit Probe Component dialog box.