### Section Cad Tolerance

This value is used by PC-DMIS to determine the hole locations in order to detect holes from CAD data. If the distance between any two surface boundary points is less than the tolerance distance, PC-DMIS will consider this a continuous surface and scan into the hole. If the distance is greater than the tolerance, PC-DMIS will assume that there is a hole between the surfaces, and during the learning process it will skip the hole.

Entry Name: SectionCadTolerance

Entry Type: Real Number specifying tolerance. Default value is 0.01.