### Auto Shutter Time To Fire

This value provides the delay (in milliseconds) that PC-DMIS waits before issuing the point detect command when PC-DMIS detects that the ROI (Region of Interest) is ready to fire. This delay gives the stage a chance to settle before firing the point detection. This value is only evaluated for the first region of interest ROI. Subsequent ROIs are evaluated with the "AutoShutterTimeToFireNth" value.

This value is only evaluated when "AutoShutterEnable" is set to TRUE (1). If the stage is not stable, then point detection is not reliable.

This value relates to the Movement Feature settle in the Live View Setup dialog box. See the "Setting up the Live View" topic in the PC-DMIS Vision documentation.

Entry Name: AutoShutterTimeToFire

Entry Type: Whole Number to specify milliseconds. Default value is 3000.