### Laser Type

This setting is responsible for selecting one of the possible laser probes - Focus Laser Sensor (FLS) or Chromatic Whitelight Sensor (CWS).

Entry Name: Laser_Type

Entry Type: 0 (zero) is the default value and indicates that no laser probes are defined in the system. 1 indicates an FLS laser probe type. 2 indicates a CWS laser probe type.

CAUTION: Please do not change this setting. Refer to the Machine Interface Installation Manual (MIIM) for detailed information.