### DCC Use Auto Move

Allows you to define the default value for the Auto Move option that will be used when an Auto Feature is created. Auto Move commands can be inserted before, after or both for the created feature. The probe will move to a distance (DccAutoMoveDistance) above the centroid or first hit and last hit of the feature being created. This value is used for Contact probes while the "AutoMove" value is used for Vision and Laser probes.

Entry Name: DCCUseAutoMove

Entry Type: Whole Number to specify move type. Default value is 0.

Value Key:

0 | None
1 | Both
2 | Before
3 | After