### Enable Rotary Absolute Position

This setting is responsible for processing the return value of the GETPOS call, providing Firmware Distributed Controller (FDC) rotary tables the ability to move through 0 and 360 degree positions when used with the EnableRotaryClockMode setting.

Note: This setting is disabled if the registry key EnableRotaryClockMode is set to False.

Entry Name: EnableRotaryAbsolutePosition

Entry Type: If set to TRUE (default), this enables FDC rotary tables to cross the 0 and 360 degree positions. In combination with EnableRotaryClockMode=TRUE, the properties for SHORTEST, CW and CCW in a Part Program rotary move through these positions are allowed.

If set to FALSE, moves through the 0 and 360 degree positions are not allowed.

Note: It is recommended that for Firmware Distributed Controller (FDC) rotary tables, the EnableRotaryAbsolutePosition and EnableRotaryClockMode registry keys should both be set to TRUE.

CAUTION: Please do not change this setting. Refer to the Machine Interface Installation Manual (MIIM) for detailed information.

More

EnableRotaryClockMode