### Color Map Validate Cad Normals

When this value is set to TRUE (1), PC-DMIS will correct CAD surface normals and make them consistent when creating a face colormap, or point colormap. For a solid, all normals are oriented outside of the material. For non-solid models normals of adjacent faces are oriented in the same direction.

Entry Name: ColorMapValidateCadNormals

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.