### External Rotab Move Min Delta

Represents the minimum angular change in degrees for an external rotary table for which PC-DMIS would issue a new requested rotary table movement. If a requested move position would be within the angle from the current table position it is considered to be already in position and the move is not actually sent to the controller for the table.

Entry Name: ExternalRotabMoveMinDelta

Entry Type: Real Number specifying angle in degrees. Default value is 0.5.