### Temp Comp Automatic

This option determines the method that will be used for Temperature Compensation.

Entry Name: TempCompAutomatic

Entry Type: Whole Number to specify the Compensation Method. Default value is 0.

U ser permission is

The following are the available compensation methods and their respective processes in PC-DMIS.

Value | Method | Process
0 | Manual | Compensation is manual.
1 | Read Temperatures from Controller | PC-DMIS reads the current temperatures from the controller automatically rather than you supplying the data.
2 | Controller Compensates Axes Only | The controller performs compensation of the machine axes itself.
3 | Controller Comps Axes and Part | The controller performs compensation of both the machine axes and the part.