### DCC Set Nom Axis

Allows you to define the default value for the Set Nom Axis option that will be used when an Auto Feature is created. When this value is set to TRUE (1), PC-DMIS will update (or "set") the nominal point location and the nominal approach direction before each execution. Also, with this option ON, the CAD surfaces will be pierced along that axis. Otherwise, the update vector will be used.

The axis (or vector) selected tells PC-DMIS along which axis (or vector) the CAD surface will be pierced to find a new theo and target.

Entry Name: DccSetNomAxis

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.