### FLS Present

Focus Laser Sensor (FLS) is a sensor for Vision machines in which a laser beam works through a lens (this assumes a camera sensor and implies that the laser beam is visible in the PC-DMIS Live view). The inherent advantage is that you can use the laser as a pointer for rapid locating of features on the part.

Entry Name: FLSPresent

Entry Type: Valid values are True and False: True will enable FDC to handle the FLS; the default value False will prevent the FLS command from being passed on to the FDC.

In order to use FLS with FDC, the following registry settings are necessary:

- (FDC) FLSPresent = True

- (MSI) Laser_Type = 1

CAUTION: Please do not change this setting. Refer to the Machine Interface Installation Manual (MIIM) for detailed information.