### End Angle 2

Use the DccEndAng2 value to affect this change rather than this value. This value is not currently used.

This value allows you to define the default value for the End Angle option that will be used when an Auto sphere is created. This is a user supplied angle in decimal degrees. This field will accept values between 0° and 90°. If the ending angle is 0°, the last row will be a single hit at the top of the sphere.

Entry Name: EndAngle2

Entry Type: Real Number to specify the angle in degrees. Default value is None ( ).

Note: It is important that the ending angle is not at more than 90°. The risk of the probe shank hitting the part is increased when a greater angle is used.

Note: When entering starting and ending angles, remember that the IJK vector always looks down the centerline, and that PC-DMIS measures DCC spheres in a counterclockwise direction.