### Readout Display Bkgr Color

This color refers to the background color for the Readout Window.

Entry Name: ReadoutDisplay BkgrColor

Entry Type: Unsigned Integer specifying decimal color number. Default value is 0 (black).

Note: It is best to alter this value inside of PC-DMIS from the Probe Readout Setup dialog box accessed by right-clicking on the Probe Readout window and selecting Setup... or selecting the Edit | Preferences | Probe Readout Setup... menu option.