### PTP_Spacer

Use the DccSpacer value to affect this change rather then this value. ???? There are now values for each feature type. How are these used versus the DccSpacer value that is shown as a reference.

Defines the distance from the nominal point location that PC-DMIS will use to measure a plane if sample hits are specified.

Entry Name: Spacer

Entry Type: Real Number to specify distance. Default value is 0.

If no value is entered, PC-DMIS uses a default distance.