### MScan Dialog 3D

This option allows you to move the probe in any direction. PC-DMIS takes a point each time you reach the increment distance between the previous point and the current point. This option is very useful when scanning using free-moving manual CMMs whose axes cannot be locked.

Entry Name: MScanDialog3D

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.