### Dimension 132 Columns

This option controls the printing format of feature locations in the inspection report. When this value is set to TRUE (1), PC-DMIS will print all feature locations in a 132 column format.

Entry Name: Dimension132Columns

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.

The following describes the columns in the 132 column printout format:

Column 1 to 10:X nominal
Column 11 to 20:X measured
Column 21 to 28:X deviation
Column 31 to 40:Y nominal
Column 41 to 50:Y measured
Column 51 to 58:Y deviation
Column 61 to 70:Z nominal
Column 71 to 80:Z measured
Column 81 to 88:Z deviation
Column 91 to 100T error (normal to surface error)
Column 101 to 101Out of Tol flag "*"
Column 104 to 105Feature type
Column 108 to 117Feature ID
Column 118 to 127Measured Diameter if any