### Force Part Alignment In Car Body

When this option is set to TRUE (1), PC-DMIS will always leave the part alignment origin at the location of the CAD model origin. Normally in PC-DMIS the part alignment origin and axes can be different than the CAD model origin and axes.

Entry Name: ForcePartAlignmentInCarBody

Entry Type: Whole Number to specify TRUE (1) or FALSE(0). Default value is None (0).