### Enable Rotary Clock Mode

This setting enables support of direction flags with Firmware Distributed Controller (FDC) rotary tables.

Note: Full support of the direction flags on FDC rotary tables requires that EnableRotaryAbsolutePosition also be set to TRUE (the default setting).

Entry Name: EnableRotaryClockMode

Entry Type: Set to TRUE (default) this enable FDC rotary tables to support the direction flags if the move does not cross the 0 degree position with the specified move direction. In combination with EnableRotaryAbsolutePosition = TRUE, the rotary move properties for SHORTEST, CW and CCW are supported.

If set to FALSE, the rotary will not support direction flags and it will not make a move through the 0 degree position, but instead move in the opposite direction to reach the destination.

Note: It is recommended that for FDC rotary tables, the EnableRotaryAbsolutePosition and EnableRotaryClockMode registry keys should both be set to TRUE.

CAUTION: Please do not change this setting. Refer to the Machine Interface Installation Manual (MIIM) for detailed information.

More

EnableRotaryAbsolutePosition