### Read Pos Updates XYZ Even If RMeas

When using Read Pos for Auto Features, this entry lets you specify whether or not a Find Hole's Read Position operation returns not only the X and Y axes, but also the Z axis, even if the auto feature uses an RMEAS feature.

You generally won't use this option. Consider this example situation: You have a contoured part which you only Rmeas to the X axis. Your Z may be out of tolerance by a large amount. Normally, you would Rmeas to Z as well, but since you don’t have a decent non-contoured feature to Rmeas to, in this case, you would need Read Pos to update X,Y, and Z.

If you set this entry to TRUE, then PC-DMIS's read position operation also includes the Z axes even if you use an RMEAS feature. If set to FALSE, then PC-DMIS behaves as it always has, using only the X and Y axes.

Entry Name: ReadPosUpdatesXYZEvenIfRMeas

Entry Type: True/False value. Default value is FALSE.