### Probe Use Wrist Map

Determines whether or not PC-DMIS uses a wrist map (also known as an "error map") file when calibrating AB angle tips on probe configurations that use an indexable wrist. When this value is set to TRUE (1), PC-DMIS will search for the wrist map file (a file named abcomp.dat) on your computer, and if found, will compensate for the wrist's error data when calibrating the AB angle tips.

Entry Name: ProbeUseWristMap

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1.

For information on creating the wrist map file, see the "Calculate Error Map" topic from the "Using a Wrist Device" section.