### DCC Angle Exterior

Defines the angle as either interior or exterior. Interior angles have the solid angle of the part less than 180°, while exterior angles are greater than 180°. With the exterior option enabled, PC-DMIS will measure the angle as exterior. It is very important to make sure this option is set correctly because of the differences in measurement sequence for each type.

Entry Name: DCCAngleExterior

Entry Type: Whole Number to specify Exterior(1) or Interior(0) angle. Default value is 1.