### Client Is Holos

Bit coded values that perform the following operations:

- Bit 0 (value 1) = Does not send or use the A0B0 angle. Also forces the UseWristStrategy key to be set for the ToolName key if a wrist device is involved.

- Bit 1 (value 2) = Forces the system to not send or use A0B0 angle for the ToolName key and is independant of whether a wrist device is used or not. It also forces the UseWristStrategy key to be set.

- Bit 2 (value 4) = Prevents sending E-Stops or similar code 8000 by dozens if machine remains in E-Stop state, or error reoccurs every second.

- Bit 4 (value 8) = Introduce a delay of value HolosSlowDown ms before sending ACK (&) / END (%)/error answer.

Entry Name: ClientIsHolos

Entry Type: Bit coded integers of 0 (zero), 1, 2 or 4. The default value is 0.