### Row Overscan

This value how far beyond the nominal feature’s dimensions the probe will scan along both the major and minor axis of the feature. If you are measuring features whose actual location may vary significantly from their theoretical values, you will need to increase this value in order to ensure that PC-DMIS measures the entire feature.

Entry Name: RowOverscan

Entry Type: Real Number to specify distance. Default value is 2.