### DCC End Ang2

Allows you to define the default value for the End Angle option that will be used when an Auto sphere is created. This is a user supplied angle in decimal degrees. This field will accept values between 0° and 90°. If the ending angle is 0°, the last row will be a single hit at the top of the sphere.

Entry Name: DccEndAng2

Entry Type: Real Number to specify the angle in degrees. Default value is 90.

Note: It is important that the ending angle is not at more than 90°. The risk of the probe shank hitting the part is increased when a greater angle is used.

Note: When entering starting and ending angles, remember that the IJK vector always looks down the centerline, and that PC-DMIS measures DCC spheres in a counterclockwise direction.