### Slave Temp Sensor Numbers (0-3)

The Slave Sensor Numbers values contain a list of one or more sensor numbers to be used for the given axis or part for the slave arm of a dual arm configuration. These values are very important when reading temperatures from the controller because they must correspond to how the sensors are actually configured.

- Each sensor is a number in the range of 1 to 32.

- Items in the list can be either a single number or a range from first to last.

- Items are separated by either commas or left blank.

- The input allows up to 32 values for any axis or the part.

Entry Name: SlaveTemp SensorNumbers(0-3)

Entry Type: Character String specifying sensor number. Default value is None ( ).

Number Key:

0 | X Axis
1 | Y Axis
2 | Z Axis
3 | Part

Note: For "manual" mode these numbers are relatively meaningless but at least one sensor number must be assigned for each axis and the part.