### Laser Circle

Circle Auto Feature

To create a laser auto circle:

1. Access the Auto Features dialog box, and select Circle.

2. Do one of the following:

1. Perform clicks on the cad to give the circle a location and vector. Then manually enter any remaining information.

2. Move the machine to the circle location using the Laser View tab of the Graphics Display Window. Next, Click the Read Point from Position button. Then manually enter the any remaining information like the diameter, depth, etc.

3. Manually enter all of the theoretical x, y, z, i, j, k, diameter, depth, etc.

3. Enter the necessary information in the Probe Toolbox tabs. You will likely want to cycle through the Laser Scan, Laser Filtering, and Laser Clipping, properties tabs to enter the information.

4. Click the Test button if desired. Warning: The machine will now move!

5. Click the Create button and then Close.

Currently, you can only measure inner circles (holes) with laser probes.

More:

Circle Specific Parameters

Circle Command Mode Text

Auto Circle Paths