<?xml version="1.0" encoding="utf-8"?>
<glossary version="1.0">
	<glossentry>
		<glossterm>6DoF</glossterm>
		<glossdef>Six Degrees of Freedom</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>ADM</glossterm>
		<glossdef>Absolute Distance Meter</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Birdbath</glossterm>
		<glossdef>Your reflector can be attached to this known position via a magnetic connector located on the front of the laser tracker.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>DRO</glossterm>
		<glossdef>Display Readout</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Hardstop</glossterm>
		<glossdef>A physical holder against which the arm rests when not in use.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>ID</glossterm>
		<glossdef>Inside Diameter</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>IFM</glossterm>
		<glossdef>Interferometer</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Nivel</glossterm>
		<glossdef>Inclination sensor designed to be used with Leica Laser Tracker. This device attaches to the laser tracker to establish orientation to gravity or monitor tracker stability.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Normal Hit</glossterm>
		<glossdef>A "Normal Hit" is taken when press and release the hit button in the same location.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>OD</glossterm>
		<glossdef>Outside Diameter</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Pulled Hit</glossterm>
		<glossdef>Changes the vector to that of the line between the location where you first depress the hit button (at the "Normal Hit" location) to the location where you release the hit button. This line must be longer than the Use Vector Distance to successfully register a "Pulled Hit".</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>RMS</glossterm>
		<glossdef>Root Mean Square</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>TCU</glossterm>
		<glossdef>Tracker Control Unit</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>TTP</glossterm>
		<glossdef>Touch-Trigger Probe</glossdef>
	</glossentry>
</glossary>
