## Leica Tracker Interface

The parameters that control how PC-DMIS interfaces with the Leica interface can be configured by selecting the Edit | Preferences | Machine Interface Setup menu item. This opens the Machine Options dialog box. The following seven tabs are available:

- Options tab

- Reset tab

- Sensor Configuration tab

- Environmental Parameters tab

- Level To Gravity tab

- System Information tab: Displays information for your configured Leica system. Included values are: IP Address, Tracker Type with Serial # (if available), Controller Type, T-CAM Type and Serial # (if available), emScon version, TP-Firmware version, Bootdriver version, and Nivel Type and Serial # (if available).

- Debug tab: See the "Generating a Debug File" topic in the Core PC-DMIS documentation.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM). Also review the documentation that came with you Leica Tracker.