## Probe Trigger Options

Using Probe Trigger Options allows you to trigger a hit when certain conditions are met while using manual CMM machines. The interfaces that support probe trigger options include: Romer, Leica, BackTalk, Faro, Garda, GOM (Krypton), Axila, Polar, and SMXLaser.

Inserting POINT AUTOTRIGGER, PLANE AUTOTRIGGER, and POINT MANUAL TRIGGER commands into your part program can be done from the Probe Trigger Options tab of the Parameters dialog box (Edit | Preferences | Parameters or F10) or from the Probe Mode toolbar.

These trigger commands function with the following supported features:

- Auto Features: Circle, Ellipse, Edge Point, Round Slot, Square Slot, Notch Slot, and Polygon

- Measured Features: Circle, Line, and Round Slot

The available Probe Trigger options are:

- Point AutoTrigger

- Plane AutoTrigger

- Point Manual Trigger