## Axila Arm Interface

The Axila interface is used with an Axila arm machine. PC-DMIS software should be installed first, before proceeding with installing driver and arm-specific data delivered with your machine. The GDS driver for your Axila machine is protected by an HASP dongle that you must attach to your computer. The GTech/ROMER CD-ROM provides utilities for use with your machine.

Before starting PC-DMIS, rename the axila.dll to interfac.dll.

The Machine Option dialog box has two tabs for the Axila interface:

Debug tab

See the "Generating a Debug File" topic.

GDS Setup tab

This tab provides a button (Start Setup) that initiates the setup software that you installed with your Axila interface.

Note: The GDS document for the Axila interface is available from the Wilcox FTP site: ftp://ftp.wilcoxassoc.com/docs/How To Docs/E121 Gds manual UK.pdf

Axila Pulled Hit Feature

The Axila interface supports pulled hits. See "Pulled Hits Method" in the "Probe Compensation" chapter.