## Probe Readout

The Probe Readout primarily displays the XYZ probe location. The display of the Probe Readout can be toggled from the Portable toolbar or by pressing and holding the portable arm left button for greater than 1 second. Pressing and holding the portable arm left button for greater than 1 second when the Probe Readout is already open will display the "T" value in the Probe Readout. The "T" value provides the distance to the CAD nominal.

When working with Build / Inspect mode, the tolerance colors used in Probe Readout indicate whether the current location is in or out of tolerance. The following colors are used:

- In Tolerance: Green

- Out-of-tolerance negative: Blue

- Out-of-tolerance positive: Red

For more information about the Probe Readout window, see the "Using the Probe Readout Window" in the "Using Other Windows, Editors, and Tools" chapter in the PC-DMIS Core documentation.