### Total Station Status Bar

The Total Station status bar automatically appears when you launch PC-DMIS Portable with the Total Station interface:

Total Station Status Bar

By using the View | Status Bar menu item you can change the status bar's size and visibility.

1. System Laser Status Indicator: This field is used to indicate the status of the system. When online the status will change depending on current settings and operations being performed.

2. Probe Name: This lists the name of the active probe.

3. Probe Diameter: This displays the probe's diameter.

4. Probe Compensation: This indicates whether probe compensation is turned ON or OFF.

5. Probe Mode: The probe mode pane will update the icon and text to reflect the currently active probing mode. The probe mode icons are the same ones that are used in the menu and the toolbar.

7. Active Station Indicator: Indicates which station is currently active. A double click onto the station indicator opens the Station Manager dialog box.

- Red (Not oriented): The station position is not computed yet.

- Green (Oriented) The station position has been computed.

8. Environmental Parameter Display: Shows the active environmental parameters: temperature, pressure, and humidity. If no weather station is connected, it is possible to double-click on the edit boxes to change their values.

9. Battery Level: This static icon and the text next to it reflect the current amount of power left in the battery. If the power level is between 25% and 100%, it displays a green background color. If the power level is between 10% and 25%, it displays a yellow background color. For anything 10% or less, it displays a red background color.