## Build and Inspect Toolbar

Build and Inspect Toolbar

The Build and Inspect Toolbar has buttons to determine how the Build and Inspect modes are used in PC-DMIS Portable. The following options are available:

Inspect / Build mode: | By default (Inspect mode), PC-DMIS displays the deviation (T) as 'Difference = Actual - Nominal'.

- Build Mode: The general purpose is to provide real-time deviations between a real object and its nominal data or CAD model. This allows you to position your part as it relates to the CAD design data.

Selecting this option will display the distance and direction that you need to move the measured point to reach the nominal position or 'Difference = Nominal - Actual'.

Note: When you are moving the part into position, there are just real-time deviations displayed without storing any data (taking hits). After the part is positioned within a reasonable deviation (e.g. 0.1mm), you would typically measure (hits are taken) the final position of the feature.

- Inspect Mode: In this mode, the position of an object (point, line of surface, etc.) is checked and compared with design data.

Surface Inspection: | Applies the Probe Readout settings that are useful for inspecting surfaces/curves.
Point Inspection: | Applies the Probe Readout settings that are useful for inspecting points.
Distance to closest feature: | When this option is enabled, the distance to the closest feature is displayed in the Probe Readout.
Show Deviation Arrow: | When this option is enabled, arrows are displayed in the Graphics Display window according to the inspect mode. The arrows are placed at the probe location in inspect mode (default) or at the measured point during build mode.