#### Joystick

If your system supports a joystick, you should use the joystick for fast adjustment of the optical probe. Use the Joystick Speed and Joystick Z Speed boxes to specify the speed used to drive the Vision probe into range of the video measurement. Speed is measured in terms of millimeters per second. The maximum or minimum values that you should use depend on your specific system. Consult your optical measuring system’s documentation for any speed restrictions.