#### Vision Round Slot

To create a Vision Round Slot:

1. For machines supporting DCC motion, select DCC Mode if you want to create and measure round slots in DCC mode.

2. Select Auto Round Slot from the Auto Feature toolbar. You can also select the Insert | Feature | Auto | Round Slot menu option. This opens the Auto Feature (round slot) dialog box.

Vision Round Slot Auto Feature dialog box

3. With the Auto Feature dialog box open, select a round slot in one of two ways:

- CAD Selection Method - From the Cad View, click once near the edge of the round slot on the CAD surface to establish the round slot's location.

- Target Selection Method - From the Live View, click three points on the first arc, and then three more points on the opposite ended arc. This establishes the round slot's location. Adjust the lighting and magnification as needed.

Important: Click as close as possible to the CAD element to ensure the PC-DMIS will not choose an incorrect element.

4. PC-DMIS Vision automatically places the nominal data for the round slot into the Auto Feature dialog box. The hit targets will automatically be displayed for the round slot.

5. Adjust the nominal information in the Auto Feature dialog box to match the theoretical values of the round slot. Also, adjust the values of the Probe Toolbox as needed.

6. Click Test to test round slot measurement.

7. Click Create on the Auto Feature dialog box to add the round slot to the part program.

8. Save the part program for future execution. See "A Note on Executing a Vision Part Program".