# Using the PC-DMIS Vision Measuring System

PC-DMIS Vision: Introduction

Factors for Measuring with PC-DMIS Vision

Understanding Targets in PC-DMIS Vision

Getting Started

Calibrating Vision Probes

Setting Machine Options

Available Vision Setup Options

Using the Graphics Display Window in PC-DMIS Vision

Using the Probe Toolbox in PC-DMIS Vision

Using Vision Gages

Creating Alignments

Measuring Auto Features with a Vision Probe

Using AutoTune Execution

Using On Error Commands

Using the Image Capture Command

Appendix A: Troubleshooting PC-DMIS Vision

Appendix B: Adding a Ring Tool

Appendix C: Using the NC-100 Video Probe

Appendix D: Using a Single uEye Camera to Create Multiple "Virtual" Cameras