### Machine Options: Wrist tab

Machine Options dialog box—Wrist tab

The Wrist tab allows you to specify the communications port and settings used to connect your computer to your optical measuring device’s wrist controller. This is for dedicated vision machines that have PH9 type wrist fitted and the Wrist portlock option selected (e.g. Mycrona).

CMM-V Note: On a CMM-V, this tab will not be available as the wrist control is done through the existing CMMI interface.