<?xml version="1.0" encoding="utf-8"?>
<glossary version="1.0">
	<glossentry>
		<glossterm>CCD</glossterm>
		<glossdef>Charge Coupled Device - This is one of the two main types of image sensors used in digital cameras.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>CMMI</glossterm>
		<glossdef>Standard CMM Interface such as a LEITZ.DLL</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Fiducials</glossterm>
		<glossdef>A point of reference. For example, In the case of a CAD file of a circuit board, these fiducials reference the location of soldering. These references may not exist in the CAD file.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Field of View</glossterm>
		<glossdef>The FOV represents the view through the video camera. In the Live View, the FOV is everything you see. In the CAD View, PC-DMIS Vision represents the FOV by a green rectangle that appears on top of the graphical image.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>FOV</glossterm>
		<glossdef>Field of View</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>HSI</glossterm>
		<glossdef>Hardware Specific Interface</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Image Tear</glossterm>
		<glossdef>This is where "breaks" in the image occur due to the refresh rate not keeping up with the speed of movement.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Intensity Circle</glossterm>
		<glossdef>The circle that is located in the middle of the Top light, Bottom light or segment of a ring light that shows the current intensity value for that light.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>MSI</glossterm>
		<glossdef>Multi Sensor Interface</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>NA</glossterm>
		<glossdef>Numerical Aperture (NA) is a measure the light-gathering ability of a Vision device. NA is a measure of the number of highly diffracted image-forming light rays captured by the objective. Higher values of numerical aperture allow increasingly oblique rays to enter the objective front lens, producing a more highly resolved image.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Par-centricity</glossterm>
		<glossdef>When the Focal XY Center of the optics is aligned with the Video Frame center through the zoom range.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Par-focality</glossterm>
		<glossdef>When the focal clarity is consistent through the zoom range.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>ROI</glossterm>
		<glossdef>Region of Interest -  Targets are divided into multiple regions based upon the Field of View. Point detection will be determined for each ROI</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Target</glossterm>
		<glossdef>Individual regions that are used for point detection for the specified feature.</glossdef>
	</glossentry>
	<glossentry>
		<glossterm>Tracker</glossterm>
		<glossdef>The visual user interface to features that control the size of the circle, start angle, end angle, and orientation.</glossdef>
	</glossentry>
</glossary>
